Barcode Error Listing Report

The Barcode Error Listing Report is available in the Barcode Report tab and it lists barcode quality errors and warnings.
Barcode location errors are displayed once for each detected type of location error.  If barcode location errors are overwritten by the operator, MERLIN regenerates this report and displays it without the barcode location errors. 
All bar error categories have three possible categories for each error.  One category for pieces with one or more error codes – upper case letters (i.e. J Error – error description), one for pieces that failed due to excessive warnings- lower case letters (i.e. j Warning Failures (11+)) and another category for pieces that contained one or more warnings, but not enough to fail (j Warnings (5+)).  Global errors have only two categories, one for any errors and one for any warnings.
There are five different sections on the report to show for the error categories described above. The section headings are:
•	Failed Automation Rate barcode with one or more Errors  
•	Failed Automation Rate barcode with (11+) Warnings
•	Automation Rate barcode per-Bar Warnings, No failure (5+)
•	Global warnings, No failure (1+)
•	Barcode Location Errors