Automation Rate Barcode Components Report

The Automation Rate Barcode Components Report is available in the Barcode Report tab and it will display up to four binary barcode images of the mailpieces for each error type as listed in the report legend.

Expanded Barcode Readability Report
Report Tag	P1	Description	Source	
Permit Number	Y	Permit Number of this Mailing.	The Permit Number entered on the Permit Information screen in the GUI.	
Mailing Date		The date of the mailing.	The Mailing Date field on the Mailing Profile screen in the GUI.	
Mail Type		The type of mail.	The type of mail being processed.	
Readability	Y	The Percentage of Good mail pieces out of the total mail pieces.	The number of good mail pieces divided by the number of mail pieces multiplied by 100.	
Pieces Analyzed		The total number of pieces analyzed for barcode quality in this evaluation run	This field is made up of three subcategories:
•	Non-IMb Pieces Analyzed
•	IM Barcode Pieces Analyzed
•	Missing or Not Decoded Barcode	
MPID		The Mail Piece Identification Number of this problem mail piece.	This is the Identification number sprayed on every piece as it passes through the machine.  This is the exact ID number of a mail piece that MERLIN determined to have a barcode problem.	
Barcode image		Barcode images with error codes.	Up to four mail piece images for each error type.	
Error Type		Error type.	Error type listed in legend.